**CENTRALISED MECHANICAL EXTRACT VENTILATION (MEV)**

**Optional General Introduction**

A continuously running Centralised Mechanical Extract System shall be installed accordance with the manufacturer’s instructions. A comprehensive system design incorporating design commissioning data shall be supplied to the installer by the manufacturer detailing the layout and all system components. The installer shall follow the design using the recommended components and shall provide completed installed performance test documentation.

All designs and installations shall meet with the requirements of Building Regulations and the NHBC Standard Chapter 8.1 – Installation.

**Product Specific Text**

**CME3 Q Plus HA – Consultant Specification**

The unit must be securely fixed to a single smooth flat surface. The base shall have circular ports allowing the direct connection of Ø100mm or Ø125mm ducting. The unit shall also incorporate zero volt boost switching with an adjustable boost Timer Overrun and an optional adjustable automatic Humidity boost facility which shall be set in accordance with client instructions at commissioning stage.

The CME shall be made using Talc Filled Polypropylene finished in two tone grey measuring (excluding ports) 310mm wide x 340mm long x 252mm high and weighing max 5kg. The CME unit shall be SAP Q qualified and capable of a SFP down to 0.16w/l/s. All CME Units shall be CE certified and manufactured under BS EN ISO 9001 and BS EN ISO 14001 and have a 3 year parts and labour guarantee.

Unit to be terminated externally using the Titon FireSafe® Air Brick/Titon Q Plus High Flow Brick (delete as appropriate) to ensure performance is not compromised.